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                                                              Extron DVS 605 Scaler Switcher

ITM Components, Dorset, are the global leading distributor of Extron Electronics, leading manufacturer of professional audio video equipment. Now Extron have released, the latest five-input HDMI Scaler with Seamless Switching. This item is available for immediate purchase with ITM Components.

Extrons DVS 605 is a high performance video scaler that includes three HDMI 1.3-compatible inputs, two universal analog video inputs with auto-format detection, and simultaneous HDMI and analog high resolution outputs. The DVS 605 accepts a wide variety of video formats including HDMI with HDCP, HDTV, RGB, and standard definition video. It features advanced Extron video signal processing with 1080i deinterlacing, Deep Colour processing, and true seamless switching for professional-quality presentations.

DVS 605 features a flexible PIP picture-in-picture mode that allows any two video sources connected to inputs 1 to 4 to be shown on one display. Several PIP (Picture-in-Picture) presets are available, including side-by-side windows, and the PIP window can be dynamically sized and positioned anywhere in the image. The DVS 605 also easily integrates analog video sources, with two universal inputs that automatically detect incoming signal formats without user intervention.   

All DVS 605 models provide lip sync delay and level adjustments for embedded HDMI audio. The DVS 605 A and DVS 605 AD add five input audio switching to accompany incoming video sources, as well as audio breakaway. With HDMI audio embedding and de-embedding, DVS 605 audio models can embed any input audio signal onto the HDMI output, and extract HDMI audio to analog captive screw and digital S/PDIF outputs. The DVS 605 AD, with audio switching plus 3G-SDI/HD-SDI output can embed two-channel audio onto the SDI output.

For further information visit http://www.itm-components.co.uk/iqs/dbitemid.2179/sfa.view/cpti.851/video_presentation_scaler_switchers.html  or call ITM Components on (01202) 872771.



Related Information:
ITM Components website: www.itm-components.co.uk 
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